IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [DesignTransferView_V1.0]"
File name: "91464-vk-sk-01.ifc"
Time stamp: "2026-03-05T08:45:58"
Author: "Gebruiker"
Organization: "BIMDeX"
Preprocessor: "BIMDeX 25.0.0.2"
Originating system: "BIMDeX"
Application: "Creo Parametric 12.4.0.0" version "12.4.0.0" identifier "Creo" by Organization "BIMDeX"

People and organizations
  Person "Gebruiker" of Organization "BIMDeX"
  Owner history of Person "Gebruiker" of Organization "BIMDeX" | application "Creo Parametric 12.4.0.0" version "12.4.0.0" identifier "Creo" by Organization "BIMDeX" | change ADDED | created 0 (1970-01-01T00:00:00Z) | last modified 1772700359 (2026-03-05T08:45:59Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  SOLIDANGLEUNIT: STERADIAN
  PLANEANGLEUNIT: RADIAN
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN
  MASSUNIT: KILO GRAM
  VOLUMEUNIT: CUBIC_METRE
  MASSDENSITYUNIT: derived

Spatial structure
IFCPROJECT "Default Project" | phase "Project Status" | description "Description of Default Project"
  IFCSITE "Default Site"
    IFCBUILDING "Default Building" | description "Description of Default Building"
      IFCBUILDINGSTOREY "Default Storey" | description "Description of Default Building Storey"
        contains 18 elements
          18 x IFCBUILDINGELEMENTPROXY | object type "General" | names: "©91464-010001", "©91464-020001", "©91464-030001" (+15 more) | property sets: PTC_Identity Data

Property sets
  PTC_Identity Data | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    COLOR = "-" (IFCTEXT)
    FINISH = "-" (IFCTEXT)
    MATERIAL = "Pine FSC" (IFCTEXT)
    PTC_MASTER_MATERIAL = "PINE_FSC" (IFCTEXT)
    PTC_MATERIAL_NAME = "PINE_FSC" (IFCTEXT)
    PTC_MP_IMP_AREA = 69192. (IFCREAL)
    PTC_MP_IMP_COGX = -6.87263E-16 (IFCREAL)
    PTC_MP_IMP_COGY = -2.42252E-14 (IFCREAL)
    PTC_MP_IMP_COGZ = -2.17271E-17 (IFCREAL)
    PTC_MP_IMP_VOLUME = 419580. (IFCREAL)
    PTC_MP_VAL_IMP_AREA = 69192. (IFCREAL)
    PTC_MP_VAL_IMP_COGX = 0. (IFCREAL)
    PTC_MP_VAL_IMP_COGY = -8.87862E-15 (IFCREAL)
    PTC_MP_VAL_IMP_COGZ = 6.93642E-16 (IFCREAL)
    PTC_MP_VAL_IMP_VOLUME = 419580. (IFCREAL)
    PTC_REPORTED_MATERIAL = "PINE_FSC" (IFCTEXT)
    PTC_UNITS_FORCE = "N" (IFCTEXT)
    PTC_UNITS_LENGTH = "mm" (IFCTEXT)
    PTC_UNITS_MASS = "g" (IFCTEXT)
    PTC_UNITS_SYSTEM_TYPE = "Mass length time (MLT)" (IFCTEXT)
    PTC_UNITS_TEMPERATURE = "C" (IFCTEXT)
    PTC_UNITS_TIME = "sec" (IFCTEXT)
    PTC_VAL_IMP_PART_STATUS = "OK" (IFCTEXT)
    PTC_VAL_IMP_SCORE = "PASS" (IFCTEXT)
    THICKNESS__MM__1 = "21" (IFCTEXT)
  PTC_Identity Data | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    COLOR = "Grey Spraycork (RAL7012)" (IFCTEXT)
    FINISH = "-" (IFCTEXT)
    MATERIAL = "Plywood FSC" (IFCTEXT)
    PTC_MASTER_MATERIAL = "PLYWOOD_FSC" (IFCTEXT)
    PTC_MATERIAL_NAME = "PLYWOOD_FSC" (IFCTEXT)
    PTC_MP_IMP_AREA = 243112. (IFCREAL)
    PTC_MP_IMP_COGX = -1.71936 (IFCREAL)
    PTC_MP_IMP_COGY = -2.27824E-13 (IFCREAL)
    PTC_MP_IMP_COGZ = -0.0439786 (IFCREAL)
    PTC_MP_IMP_VOLUME = 1327080. (IFCREAL)
    PTC_MP_VAL_IMP_AREA = 920623. (IFCREAL)
    PTC_MP_VAL_IMP_COGX = 0. (IFCREAL)
    PTC_MP_VAL_IMP_COGY = 0. (IFCREAL)
    PTC_MP_VAL_IMP_COGZ = 2.92476E-16 (IFCREAL)
    PTC_MP_VAL_IMP_VOLUME = 5296560. (IFCREAL)
    PTC_REPORTED_MATERIAL = "PLYWOOD_FSC" (IFCTEXT)
    PTC_UNITS_FORCE = "N" (IFCTEXT)
    PTC_UNITS_LENGTH = "mm" (IFCTEXT)
    PTC_UNITS_MASS = "g" (IFCTEXT)
    PTC_UNITS_SYSTEM_TYPE = "Mass length time (MLT)" (IFCTEXT)
    PTC_UNITS_TEMPERATURE = "C" (IFCTEXT)
    PTC_UNITS_TIME = "sec" (IFCTEXT)
    PTC_VAL_IMP_PART_STATUS = "OK" (IFCTEXT)
    PTC_VAL_IMP_SCORE = "PASS" (IFCTEXT)
    THICKNESS__MM__1 = "12" (IFCTEXT)
  PTC_Identity Data | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    COLOR = "-" (IFCTEXT)
    FINISH = "-" (IFCTEXT)
    MATERIAL = "Plywood FSC" (IFCTEXT)
    PTC_MASTER_MATERIAL = "PLYWOOD_FSC" (IFCTEXT)
    PTC_MATERIAL_NAME = "PLYWOOD_FSC" (IFCTEXT)
    PTC_MP_IMP_AREA = 196667. (IFCREAL)
    PTC_MP_IMP_COGX = -0.855771 (IFCREAL)
    PTC_MP_IMP_COGY = -16.4961 (IFCREAL)
    PTC_MP_IMP_COGZ = 0. (IFCREAL)
    PTC_MP_IMP_VOLUME = 1053070. (IFCREAL)
    PTC_MP_VAL_IMP_AREA = 196667. (IFCREAL)
    PTC_MP_VAL_IMP_COGX = -0.855771 (IFCREAL)
    PTC_MP_VAL_IMP_COGY = -16.4961 (IFCREAL)
    PTC_MP_VAL_IMP_COGZ = 8.29116E-17 (IFCREAL)
    PTC_MP_VAL_IMP_VOLUME = 1053070. (IFCREAL)
    PTC_REPORTED_MATERIAL = "PLYWOOD_FSC" (IFCTEXT)
    PTC_UNITS_FORCE = "N" (IFCTEXT)
    PTC_UNITS_LENGTH = "mm" (IFCTEXT)
    PTC_UNITS_MASS = "g" (IFCTEXT)
    PTC_UNITS_SYSTEM_TYPE = "Mass length time (MLT)" (IFCTEXT)
    PTC_UNITS_TEMPERATURE = "C" (IFCTEXT)
    PTC_UNITS_TIME = "sec" (IFCTEXT)
    PTC_VAL_IMP_PART_STATUS = "OK" (IFCTEXT)
    PTC_VAL_IMP_SCORE = "PASS" (IFCTEXT)
    THICKNESS__MM__1 = "12" (IFCTEXT)
  PTC_Identity Data | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    COLOR = "Grey Spraycork (RAL7012)" (IFCTEXT)
    FINISH = "-" (IFCTEXT)
    MATERIAL = "Larch wood" (IFCTEXT)
    PTC_MASTER_MATERIAL = "LARCH_WOOD" (IFCTEXT)
    PTC_MATERIAL_NAME = "LARCH_WOOD" (IFCTEXT)
    PTC_MP_IMP_AREA = 23065.8 (IFCREAL)
    PTC_MP_IMP_COGX = -2.48493 (IFCREAL)
    PTC_MP_IMP_COGY = -13.6466 (IFCREAL)
    PTC_MP_IMP_COGZ = 1.86227E-16 (IFCREAL)
    PTC_MP_IMP_VOLUME = 142692. (IFCREAL)
    PTC_MP_VAL_IMP_AREA = 23065.8 (IFCREAL)
    PTC_MP_VAL_IMP_COGX = -2.48493 (IFCREAL)
    PTC_MP_VAL_IMP_COGY = -13.6466 (IFCREAL)
    PTC_MP_VAL_IMP_COGZ = -2.56293E-12 (IFCREAL)
    PTC_MP_VAL_IMP_VOLUME = 142692. (IFCREAL)
    PTC_REPORTED_MATERIAL = "LARCH_WOOD" (IFCTEXT)
    PTC_UNITS_FORCE = "N" (IFCTEXT)
    PTC_UNITS_LENGTH = "mm" (IFCTEXT)
    PTC_UNITS_MASS = "g" (IFCTEXT)
    PTC_UNITS_SYSTEM_TYPE = "Mass length time (MLT)" (IFCTEXT)
    PTC_UNITS_TEMPERATURE = "C" (IFCTEXT)
    PTC_UNITS_TIME = "sec" (IFCTEXT)
    PTC_VAL_IMP_PART_STATUS = "OK" (IFCTEXT)
    PTC_VAL_IMP_SCORE = "PASS" (IFCTEXT)
    THICKNESS__MM__1 = "20" (IFCTEXT)
  PTC_Identity Data | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    COLOR = "-" (IFCTEXT)
    FINISH = "-" (IFCTEXT)
    MATERIAL = "Pine FSC" (IFCTEXT)
    PTC_MASTER_MATERIAL = "PINE_FSC" (IFCTEXT)
    PTC_MATERIAL_NAME = "PINE_FSC" (IFCTEXT)
    PTC_MP_IMP_AREA = 65016. (IFCREAL)
    PTC_MP_IMP_COGX = 5.20417E-15 (IFCREAL)
    PTC_MP_IMP_COGY = 0. (IFCREAL)
    PTC_MP_IMP_COGZ = -4.88709E-17 (IFCREAL)
    PTC_MP_IMP_VOLUME = 359640. (IFCREAL)
    PTC_MP_VAL_IMP_AREA = 65016. (IFCREAL)
    PTC_MP_VAL_IMP_COGX = 0. (IFCREAL)
    PTC_MP_VAL_IMP_COGY = 0. (IFCREAL)
    PTC_MP_VAL_IMP_COGZ = 0. (IFCREAL)
    PTC_MP_VAL_IMP_VOLUME = 359640. (IFCREAL)
    PTC_REPORTED_MATERIAL = "PINE_FSC" (IFCTEXT)
    PTC_UNITS_FORCE = "N" (IFCTEXT)
    PTC_UNITS_LENGTH = "mm" (IFCTEXT)
    PTC_UNITS_MASS = "g" (IFCTEXT)
    PTC_UNITS_SYSTEM_TYPE = "Mass length time (MLT)" (IFCTEXT)
    PTC_UNITS_TEMPERATURE = "C" (IFCTEXT)
    PTC_UNITS_TIME = "sec" (IFCTEXT)
    PTC_VAL_IMP_PART_STATUS = "OK" (IFCTEXT)
    PTC_VAL_IMP_SCORE = "PASS" (IFCTEXT)
    THICKNESS__MM__1 = "18" (IFCTEXT)
  PTC_Identity Data | properties | on 1 object (1 IFCPROJECT)
    CAD_SYSTEM = "SOLIDWORKS_ASM" (IFCTEXT)
    DEX_MASTER = "91464 - 00" (IFCTEXT)
    MODEL_DATE = "06/20/2023 15:45:05" (IFCTEXT)
    MODEL_VERSION = "N/A" (IFCTEXT)
    NATIVE_NAME = "91464 - 00" (IFCTEXT)
    PTC_MP_VAL_IMP_AREA = 5443160. (IFCREAL)
    PTC_MP_VAL_IMP_VOLUME = 31857400. (IFCREAL)
    PTC_UNITS_FORCE = "N" (IFCTEXT)
    PTC_UNITS_LENGTH = "mm" (IFCTEXT)
    PTC_UNITS_MASS = "g" (IFCTEXT)
    PTC_UNITS_SYSTEM_TYPE = "Mass length time (MLT)" (IFCTEXT)
    PTC_UNITS_TEMPERATURE = "C" (IFCTEXT)
    PTC_UNITS_TIME = "sec" (IFCTEXT)
    PTC_VAL_IMP_MISSING_COMP_COUNT = 2 (IFCINTEGER)
    PTC_VAL_IMP_SCORE = "FAIL" (IFCTEXT)
    REF_LINK = "D:\onedrive\OneDrive - Vivara Pro B.V\CAD\91464-vk-sk-01-bat-wall\91464 - 00.sld" (IFCTEXT)
    TIM_STATUS = "Up-To-Date" (IFCTEXT)
  PTC_Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    COLOR = "Grey Spraycork (RAL7012)" (IFCTEXT)
    FINISH = "-" (IFCTEXT)
    MATERIAL = "Plywood FSC" (IFCTEXT)
    PTC_MASTER_MATERIAL = "PLYWOOD_FSC" (IFCTEXT)
    PTC_MATERIAL_NAME = "PLYWOOD_FSC" (IFCTEXT)
    PTC_MP_IMP_AREA = 243112. (IFCREAL)
    PTC_MP_IMP_COGX = -1.71936 (IFCREAL)
    PTC_MP_IMP_COGY = -2.27824E-13 (IFCREAL)
    PTC_MP_IMP_COGZ = -0.0439786 (IFCREAL)
    PTC_MP_IMP_VOLUME = 1327080. (IFCREAL)
    PTC_MP_VAL_IMP_AREA = 243112. (IFCREAL)
    PTC_MP_VAL_IMP_COGX = -1.71936 (IFCREAL)
    PTC_MP_VAL_IMP_COGY = -2.13151E-13 (IFCREAL)
    PTC_MP_VAL_IMP_COGZ = -0.0439786 (IFCREAL)
    PTC_MP_VAL_IMP_VOLUME = 1327080. (IFCREAL)
    PTC_REPORTED_MATERIAL = "PLYWOOD_FSC" (IFCTEXT)
    PTC_UNITS_FORCE = "N" (IFCTEXT)
    PTC_UNITS_LENGTH = "mm" (IFCTEXT)
    PTC_UNITS_MASS = "g" (IFCTEXT)
    PTC_UNITS_SYSTEM_TYPE = "Mass length time (MLT)" (IFCTEXT)
    PTC_UNITS_TEMPERATURE = "C" (IFCTEXT)
    PTC_UNITS_TIME = "sec" (IFCTEXT)
    PTC_VAL_IMP_PART_STATUS = "OK" (IFCTEXT)
    PTC_VAL_IMP_SCORE = "PASS" (IFCTEXT)
    THICKNESS__MM__1 = "12" (IFCTEXT)
  PTC_Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    COLOR = "Grey Spraycork (RAL7012)" (IFCTEXT)
    FINISH = "-" (IFCTEXT)
    MATERIAL = "Plywood FSC" (IFCTEXT)
    PTC_MASTER_MATERIAL = "PLYWOOD_FSC" (IFCTEXT)
    PTC_MATERIAL_NAME = "PLYWOOD_FSC" (IFCTEXT)
    PTC_MP_IMP_AREA = 243112. (IFCREAL)
    PTC_MP_IMP_COGX = -1.71936 (IFCREAL)
    PTC_MP_IMP_COGY = -2.27824E-13 (IFCREAL)
    PTC_MP_IMP_COGZ = -0.0439786 (IFCREAL)
    PTC_MP_IMP_VOLUME = 1327080. (IFCREAL)
    PTC_MP_VAL_IMP_AREA = 1053730. (IFCREAL)
    PTC_MP_VAL_IMP_COGX = 1.72706E-07 (IFCREAL)
    PTC_MP_VAL_IMP_COGY = -2.22215 (IFCREAL)
    PTC_MP_VAL_IMP_COGZ = -0.0096682 (IFCREAL)
    PTC_MP_VAL_IMP_VOLUME = 6036610. (IFCREAL)
    PTC_REPORTED_MATERIAL = "PLYWOOD_FSC" (IFCTEXT)
    PTC_UNITS_FORCE = "N" (IFCTEXT)
    PTC_UNITS_LENGTH = "mm" (IFCTEXT)
    PTC_UNITS_MASS = "g" (IFCTEXT)
    PTC_UNITS_SYSTEM_TYPE = "Mass length time (MLT)" (IFCTEXT)
    PTC_UNITS_TEMPERATURE = "C" (IFCTEXT)
    PTC_UNITS_TIME = "sec" (IFCTEXT)
    PTC_VAL_IMP_PART_STATUS = "OK" (IFCTEXT)
    PTC_VAL_IMP_SCORE = "PASS" (IFCTEXT)
    THICKNESS__MM__1 = "12" (IFCTEXT)
  PTC_Identity Data: 4 more contents on 4 objects not shown